{"text_format":"3","workbook":"xls","n_sheets":24,"sheets":["0420T系列规格 ","0420TF系列","0420H系列规格","0520T系列规格","0530T系列规格","0530H系列规格","0620T系列规格  ","0624系列规格","0630系列规格","0630H系列规格","0630T系列规格","0630TF系系列规格","0640系列规格","0650系列规格","0850系列规格","1040系列规格","1040T系列规格","1050系列规格","1240系列规格","1250系列规格","1260系列规格 ","1770系列规格","2213系列规格","Sheet1"],"not_rendered":{"images":76},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"0420T系列规格 ","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[24,0,24,5],[25,0,25,5],[26,0,26,5],[27,0,27,5],[28,0,28,5]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺科技有限公司"]
["SMD POWER INDUCTORS:           FHW-0420 Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
["0420T","4.06±0.30","4.49±0.40","2.0MAX","1.1±0.3","2.0±0.3"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW-0420-R10M-G/B",0.1,{"v":11,"d":"11.0"},{"v":28,"d":"28.0"},{"v":3,"d":"3.0"},{"v":5,"d":"5.0"}]
["FHW-0420-R22M-G/B",0.22,{"v":10,"d":"10.0"},{"v":18,"d":"18.0"},4.4,{"v":6,"d":"6.0"}]
["FHW-0420-R33M-G/B",0.33,{"v":7,"d":"7.0"},{"v":12,"d":"12.0"},7.5,9.8]
["FHW-0420-R47M-G/B",0.47,5.5,{"v":10,"d":"10.0"},13.5,{"v":16,"d":"16.0"}]
["FHW-0420-R56M-G/B",0.56,{"v":6,"d":"6.0"},{"v":9,"d":"9.0"},{"v":12,"d":"12.0"},{"v":15,"d":"15.0"}]
["FHW-0420-R68M-G/B",0.68,4.5,8.5,{"v":22,"d":"22.0"},{"v":29,"d":"29.0"}]
["FHW-0420-1R0M-G/B",{"v":1,"d":"1.0"},{"v":4,"d":"4.0"},{"v":8,"d":"8.0"},{"v":25,"d":"25.0"},{"v":30,"d":"30.0"}]
["FHW-0420-1R2M-G/B",1.2,{"v":4,"d":"4.0"},{"v":7,"d":"7.0"},{"v":33,"d":"33.0"},39.6]
["FHW-0420-1R5M-G/B",1.5,{"v":4,"d":"4.0"},{"v":7,"d":"7.0"},{"v":35,"d":"35.0"},{"v":42,"d":"42.0"}]
["FHW-0420-2R2M-G/B",2.2,{"v":3,"d":"3.0"},5.5,{"v":56,"d":"56.0"},{"v":70,"d":"70.0"}]
["FHW-0420-3R3M-G/B",3.3,2.5,{"v":5,"d":"5.0"},{"v":60,"d":"60.0"},{"v":100,"d":"100.0"}]
["FHW-0420-4R7M-G/B",4.7,2.2,{"v":4,"d":"4.0"},{"v":115,"d":"115.0"},{"v":150,"d":"150.0"}]
["FHW-0420-5R6M-G/B",5.6,{"v":2,"d":"2.0"},3.5,{"v":145,"d":"145.0"},{"v":173,"d":"173.0"}]
["FHW-0420-6R8M-G/B",6.8,1.5,{"v":3,"d":"3.0"},{"v":148,"d":"148.0"},{"v":178,"d":"178.0"}]
["FHW-0420-8R2M-G/B",8.2,1.2,2.5,{"v":241,"d":"241.0"},{"v":280,"d":"280.0"}]
["FHW-0420-100M-G/B",10,1.5,2.5,{"v":278,"d":"278.0"},{"v":317,"d":"317.0"}]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 25%"]
["Note4: The packing quantity is 3000Pcs/ disk"]
[]
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"0420TF系列","index":1,"n_rows":31,"n_cols":6,"rows_kept":31,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[20,0,20,5],[21,0,21,5],[22,0,22,5],[23,0,23,5],[24,0,24,5]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺科技有限公司"]
["SMD POWER INDUCTORS:           FHW-0420TF Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
["0420TF","4.06±0.30","4.49±0.40","2.0MAX","1.1±0.3","2.0±0.3"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW-0420-R22M-C/B",0.22,{"v":10,"d":"10.0"},{"v":18,"d":"18.0"},4.5,5.4]
["FHW-0420-R33M-C/B",0.33,{"v":8,"d":"8.0"},{"v":14,"d":"14.0"},{"v":10,"d":"10.0"},{"v":12,"d":"12.0"}]
["FHW-0420-R47M-C/B",0.47,{"v":7,"d":"7.0"},{"v":13,"d":"13.0"},13.4,{"v":16,"d":"16.0"}]
["FHW-0420-R56M-C/B",0.56,{"v":6,"d":"6.0"},{"v":11,"d":"11.0"},{"v":17,"d":"17.0"},{"v":20,"d":"20.0"}]
["FHW-0420-R68M-C/B",0.68,5.5,{"v":10,"d":"10.0"},{"v":18,"d":"18.0"},{"v":22,"d":"22.0"}]
["FHW-0420-1R0M-C/B",{"v":1,"d":"1.0"},{"v":5,"d":"5.0"},{"v":9,"d":"9.0"},{"v":25,"d":"25.0"},{"v":30,"d":"30.0"}]
["FHW-0420-1R5M-C/B",1.5,4.5,{"v":8,"d":"8.0"},{"v":35,"d":"35.0"},{"v":42,"d":"42.0"}]
["FHW-0420-2R2M-C/B",2.2,{"v":3,"d":"3.0"},{"v":6,"d":"6.0"},{"v":53,"d":"53.0"},{"v":64,"d":"64.0"}]
["FHW-0420-3R3M-C/B",3.3,2.5,{"v":5,"d":"5.0"},{"v":67,"d":"67.0"},{"v":80,"d":"80.0"}]
["FHW-0420-4R7M-C/B",4.7,2.2,4.5,{"v":115,"d":"115.0"},{"v":150,"d":"150.0"}]
["FHW-0420-6R8M-C/B",6.8,{"v":2,"d":"2.0"},3.5,{"v":161,"d":"161.0"},{"v":193,"d":"193.0"}]
["FHW-0420-100M-C/B",10,1.5,{"v":3,"d":"3.0"},{"v":264,"d":"264.0"},{"v":317,"d":"317.0"}]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 30%"]
["Note4: The packing quantity is 3000Pcs/ disk"]
[]
[]
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"0420H系列规格","index":2,"n_rows":31,"n_cols":6,"rows_kept":31,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[19,0,19,5],[20,0,20,5],[21,0,21,5],[22,0,22,5],[23,0,23,5]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺科技有限公司"]
["SMD POWER INDUCTORS:           FHW-0420H Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
["0420H","4.06±0.30","4.49±0.40","2.0MAX","1.1±0.3","2.0±0.3"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW-0420-R10M-B",0.1,{"v":15,"d":"15.0"},{"v":28,"d":"28.0"},3.6,4.4]
["FHW-0420-R22M-B",0.22,{"v":7,"d":"7.0"},{"v":14,"d":"14.0"},5.3,6.4]
["FHW-0420-R33M-B",0.33,6.5,{"v":12,"d":"12.0"},{"v":8,"d":"8.0"},9.6]
["FHW-0420-R47M-B",0.47,{"v":6,"d":"6.0"},{"v":10,"d":"10.0"},{"v":14,"d":"14.0"},{"v":17,"d":"17.0"}]
["FHW-0420-R68M-B",0.68,{"v":5,"d":"5.0"},{"v":8,"d":"8.0"},{"v":17,"d":"17.0"},20.4]
["FHW-0420-1R0M-B",{"v":1,"d":"1.0"},{"v":4,"d":"4.0"},{"v":7,"d":"7.0"},{"v":26,"d":"26.0"},{"v":32,"d":"32.0"}]
["FHW-0420-1R5M-B",1.5,3.5,{"v":6,"d":"6.0"},{"v":35,"d":"35.0"},{"v":42,"d":"42.0"}]
["FHW-0420-2R2M-B",2.2,{"v":3,"d":"3.0"},{"v":5,"d":"5.0"},{"v":52,"d":"52.0"},{"v":58,"d":"58.0"}]
["FHW-0420-3R3M-B",3.3,2.5,{"v":4,"d":"4.0"},{"v":75,"d":"75.0"},{"v":90,"d":"90.0"}]
["FHW-0420-4R7M-B",4.7,{"v":2,"d":"2.0"},3.5,{"v":115,"d":"115.0"},{"v":150,"d":"150.0"}]
["FHW-0420-100M-B",10,1.5,{"v":3,"d":"3.0"},{"v":278,"d":"278.0"},{"v":334,"d":"334.0"}]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 30%"]
["Note4: The packing quantity is 3000Pcs/ disk"]
[]
[]
[]
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"0520T系列规格","index":3,"n_rows":33,"n_cols":6,"rows_kept":33,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[21,0,21,5],[22,0,22,5],[23,0,23,5],[24,0,24,5],[25,0,25,5]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺科技有限公司"]
["SMD POWER INDUCTORS:        FHW-0520 Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
[520,"5.18±0.3","5.49±0.4","2.0MAX","1.2±0.3","2.0±0.3"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW0520-R10M-G/B",0.1,{"v":13,"d":"13.0"},{"v":25,"d":"25.0"},2.1,2.6]
["FHW-0520-R22M-G/B",0.22,{"v":16,"d":"16.0"},{"v":26,"d":"26.0"},4.4,5.3]
["FHW-0520-R33M-G/B",0.33,7.5,{"v":13,"d":"13.0"},8.4,9.5]
["FHW-0520-R47M-G/B",0.47,{"v":8,"d":"8.0"},12.5,10.5,{"v":13,"d":"13.0"}]
["FHW-0520-R68M-G/B",0.68,{"v":6,"d":"6.0"},{"v":12,"d":"12.0"},{"v":14,"d":"14.0"},{"v":17,"d":"17.0"}]
["FHW-0520-1R0M-G/B",1,{"v":5,"d":"5.0"},{"v":10,"d":"10.0"},{"v":17,"d":"17.0"},19.2]
["FHW-0520-2R2M-G/B",2.2,{"v":4,"d":"4.0"},{"v":6,"d":"6.0"},{"v":32,"d":"32.0"},{"v":38,"d":"38.0"}]
["FHW-0520-3R3M-G/B",3.3,{"v":3,"d":"3.0"},4.5,{"v":58,"d":"58.0"},{"v":70,"d":"70.0"}]
["FHW-0520-4R7M-G/B",4.7,2.8,4.2,{"v":74,"d":"74.0"},{"v":96,"d":"96.0"}]
["FHW-0520-5R6M-G/B",5.6,2.5,4.2,{"v":86,"d":"86.0"},{"v":103,"d":"103.0"}]
["FHW-0520-6R8M-G/B",6.8,2.2,{"v":4,"d":"4.0"},{"v":114,"d":"114.0"},{"v":137,"d":"137.0"}]
["FHW-0520-100M-G/B",10,1.8,{"v":3,"d":"3.0"},{"v":135,"d":"135.0"},{"v":178,"d":"178.0"}]
[]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 25%"]
["Note4：The packing quantity is 3000Pcs/ disk"]
[]
[]
[]
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"0530T系列规格","index":4,"n_rows":32,"n_cols":6,"rows_kept":32,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[21,0,21,5],[22,0,22,5],[23,0,23,5],[24,0,24,5],[25,0,25,5]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺科技有限公司"]
["SMD POWER INDUCTORS:      FHW-0530T Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
["0530T","5.18±0.3","5.49±0.4","3.0MAX","1.2±0.3","2.0±0.3"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW-0530-R22M-G/B",0.22,{"v":20,"d":"20.0"},{"v":35,"d":"35.0"},{"v":4,"d":"4.0"},4.8]
["FHW-0530-R68M-G/B",0.68,{"v":7,"d":"7.0"},{"v":14,"d":"14.0"},{"v":9,"d":"9.0"},{"v":11,"d":"11.0"}]
["FHW-0530-1R0M-G/B",1,6.5,{"v":12,"d":"12.0"},{"v":12,"d":"12.0"},{"v":14,"d":"14.0"}]
["FHW-0530-1R2M-G/B",1.2,{"v":6,"d":"6.0"},{"v":10,"d":"10.0"},{"v":11,"d":"11.0"},{"v":13,"d":"13.0"}]
["FHW-0530-1R5M-G/B",1.5,5.5,{"v":10,"d":"10.0"},{"v":17,"d":"17.0"},20.4]
["FHW-0530-2R2M-G/B",2.2,{"v":5,"d":"5.0"},{"v":9,"d":"9.0"},{"v":25,"d":"25.0"},32.5]
["FHW-0530-3R3M-G/B",3.3,4.5,8.5,{"v":33,"d":"33.0"},{"v":38,"d":"38.0"}]
["FHW-0530-4R7M-G/B",4.7,{"v":4,"d":"4.0"},{"v":8,"d":"8.0"},{"v":53,"d":"53.0"},{"v":64,"d":"64.0"}]
["FHW-0530-6R8M-G/B",6.8,{"v":4,"d":"4.0"},{"v":7,"d":"7.0"},{"v":80,"d":"80.0"},{"v":100,"d":"100.0"}]
["FHW0530-100M-G/B",10,2.5,4.5,{"v":110,"d":"110.0"},{"v":132,"d":"132.0"}]
["FHW-0530-150M-G/B",15,2.5,{"v":4,"d":"4.0"},{"v":143,"d":"143.0"},{"v":163,"d":"163.0"}]
["FHW-0530-220M-G/B",22,{"v":2,"d":"2.0"},3.5,{"v":270,"d":"270.0"},{"v":324,"d":"324.0"}]
["FHW-0530-330M-G/B",33,1.2,2.5,{"v":330,"d":"330.0"},{"v":372,"d":"372.0"}]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 25%"]
["Note4：The packing quantity is 2000Pcs/ disk"]
[]
[]
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"0530H系列规格","index":5,"n_rows":29,"n_cols":6,"rows_kept":29,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[17,0,17,5],[18,0,18,5],[19,0,19,5],[20,0,20,5],[21,0,21,5]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺科技有限公司"]
["SMD POWER INDUCTORS:     FHW-0530H Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
["0530H","5.18±0.3","5.49±0.4","3.0MAX","1.2±0.3","2.0±0.3"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW0530-R47M-B",0.47,{"v":8,"d":"8.0"},{"v":14,"d":"14.0"},{"v":7,"d":"7.0"},8.5]
["FHW0530-R68M-B",0.68,{"v":7,"d":"7.0"},{"v":12,"d":"12.0"},{"v":9,"d":"9.0"},{"v":11,"d":"11.0"}]
["FHW0530-1R0M-B",{"v":1,"d":"1.0"},{"v":6,"d":"6.0"},{"v":10,"d":"10.0"},{"v":10,"d":"10.0"},{"v":12,"d":"12.0"}]
["FHW0530-1R5M-B",1.5,{"v":5,"d":"5.0"},{"v":9,"d":"9.0"},{"v":17,"d":"17.0"},20.4]
["FHW0530-2R2M-B",2.2,4.5,8.5,{"v":25,"d":"25.0"},{"v":35,"d":"35.0"}]
["FHW0530-3R3M-B",3.3,{"v":5,"d":"5.0"},{"v":8,"d":"8.0"},{"v":32,"d":"32.0"},{"v":38,"d":"38.0"}]
["FHW0530-4R7M-B",4.7,3.5,{"v":6,"d":"6.0"},{"v":52,"d":"52.0"},{"v":62,"d":"62.0"}]
["FHW0530-6R8M-B",6.8,{"v":3,"d":"3.0"},{"v":5,"d":"5.0"},{"v":83,"d":"83.0"},{"v":100,"d":"100.0"}]
["FHW0530-100M-B",10,{"v":2,"d":"2.0"},3.5,{"v":95,"d":"95.0"},{"v":115,"d":"115.0"}]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 30%"]
["Note4：The packing quantity is 2000Pcs/ disk"]
[]
[]
[]
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"0620T系列规格  ","index":6,"n_rows":32,"n_cols":6,"rows_kept":32,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[19,0,19,5],[20,0,20,5],[21,0,21,5],[22,0,22,5],[23,0,23,5]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺科技有限公司"]
["SMD POWER  INDUCTORS:     FHW-0620T Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
["0620T","6.6±0.2","7.4MAX","2.0MAX","1.6±0.3","3.0±0.2"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW0620-R10M-G/B",0.1,{"v":16,"d":"16.0"},{"v":30,"d":"30.0"},2.5,3.5]
["FHW0620-R33M-G/B",0.33,{"v":13,"d":"13.0"},{"v":24,"d":"24.0"},5.6,6.8]
["FHW0620-R47M-G/B",0.47,{"v":10,"d":"10.0"},{"v":22,"d":"22.0"},6.4,{"v":8,"d":"8.0"}]
["FHW0620-R68M-G/B",0.68,7.5,{"v":14,"d":"14.0"},{"v":10,"d":"10.0"},12.7]
["FHW0620-1R0M-G/B",{"v":1,"d":"1.0"},{"v":7,"d":"7.0"},{"v":12,"d":"12.0"},{"v":16,"d":"16.0"},19.2]
["FHW0620-1R5M-G/B",1.5,5.5,{"v":10,"d":"10.0"},{"v":26,"d":"26.0"},{"v":32,"d":"32.0"}]
["FHW0620-2R2M-G/B",2.2,{"v":5,"d":"5.0"},{"v":9,"d":"9.0"},{"v":32,"d":"32.0"},{"v":36,"d":"36.0"}]
["FHW0620-3R3M-G/B",3.3,4.5,{"v":8,"d":"8.0"},{"v":65,"d":"65.0"},{"v":78,"d":"78.0"}]
["FHW0620-4R7M-G/B",4.7,3.5,5.5,{"v":73,"d":"73.0"},{"v":88,"d":"88.0"}]
["FHW0620-6R8M-G/B",6.8,{"v":3,"d":"3.0"},{"v":5,"d":"5.0"},{"v":114,"d":"114.0"},{"v":140,"d":"140.0"}]
["FHW0620-100M-G/B",10,2,{"v":4,"d":"4.0"},{"v":147,"d":"147.0"},{"v":180,"d":"180.0"}]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 25%"]
["Note4：The packing quantity is 2000Pcs/ disk"]
[]
[]
[]
[]
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"0624系列规格","index":7,"n_rows":36,"n_cols":6,"rows_kept":36,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[23,0,23,5],[24,0,24,5],[25,0,25,5],[26,0,26,5],[27,0,27,5]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺科技有限公司"]
["SMD POWER  INDUCTORS:    FHW-0624 Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
[624,"6.6±0.2","7.4MAX","2.4MAX","1.6±0.3","3.0±0.2"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW0624-R10M-G/B",0.1,30,50,1.8,3.5]
["FHW0624-R22M-G/B",0.22,{"v":12,"d":"12.0"},{"v":21,"d":"21.0"},1.7,3.2]
["FHW0624-R47M-G/B",0.47,{"v":10,"d":"10.0"},{"v":18,"d":"18.0"},{"v":4,"d":"4.0"},6.5]
["FHW0624-R68M-G/B",0.68,{"v":9,"d":"9.0"},{"v":16,"d":"16.0"},{"v":6,"d":"6.0"},9.4]
["FHW0624-R82M-G/B",0.82,8.5,{"v":15,"d":"15.0"},8.7,11.8]
["FHW0624-1R0M-G/B",{"v":1,"d":"1.0"},{"v":8,"d":"8.0"},{"v":13,"d":"13.0"},{"v":9,"d":"9.0"},{"v":12,"d":"12.0"}]
["FHW0624-1R5M-G/B",1.5,{"v":7,"d":"7.0"},{"v":12,"d":"12.0"},{"v":14,"d":"14.0"},{"v":17,"d":"17.0"}]
["FHW0624-2R2M-G/B",2.2,{"v":6,"d":"6.0"},{"v":10,"d":"10.0"},{"v":22,"d":"22.0"},{"v":34,"d":"34.0"}]
["FHW0624-3R3M-G/B",3.3,{"v":5,"d":"5.0"},{"v":9,"d":"9.0"},{"v":29,"d":"29.0"},{"v":35,"d":"35.0"}]
["FHW0624-4R7M-G/B",4.7,{"v":5,"d":"5.0"},{"v":8,"d":"8.0"},{"v":41,"d":"41.0"},{"v":50,"d":"50.0"}]
["FHW0624-6R8M-G/B",6.8,{"v":3,"d":"3.0"},{"v":6,"d":"6.0"},{"v":52,"d":"52.0"},{"v":72,"d":"72.0"}]
["FHW0624-8R2M-G/B",8.2,2.8,{"v":5,"d":"5.0"},{"v":82,"d":"82.0"},{"v":72,"d":"72.0"}]
["FHW0624-100M-G/B",{"v":10,"d":"10.0"},{"v":2,"d":"2.0"},{"v":4,"d":"4.0"},{"v":82,"d":"82.0"},{"v":106,"d":"106.0"}]
["FHW0624-150M-G/B",15,1.5,{"v":3,"d":"3.0"},{"v":112,"d":"112.0"},{"v":135,"d":"135.0"}]
[]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 30%"]
["Note4：The packing quantity is 2000Pcs/ disk"]
[]
[]
[]
[]
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"0630系列规格","index":8,"n_rows":40,"n_cols":6,"rows_kept":40,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[28,0,28,5],[29,0,29,5],[30,0,30,5],[31,0,31,5],[32,0,32,5]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺科技有限公司"]
["SMD POWER  INDUCTORS:        FHW-0630 Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
[630,"6.6±0.2","7.4MAX","3.0MAX","1.6±0.3","3.0±0.2"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW0630-R10M-G/B",0.1,{"v":20,"d":"20.0"},{"v":40,"d":"40.0"},1.6,{"v":2,"d":"2.0"}]
["FHW0630-R22M-G/B",0.22,{"v":18,"d":"18.0"},{"v":34,"d":"34.0"},2.1,{"v":3,"d":"3.0"}]
["FHW0630-R33M-G/B",0.33,{"v":16,"d":"16.0"},{"v":30,"d":"30.0"},2.4,3.5]
["FHW0630-R47M-G/B",0.47,{"v":15,"d":"15.0"},{"v":22,"d":"22.0"},3.1,{"v":4,"d":"4.0"}]
["FHW0630-R68M-G/B",0.68,{"v":13,"d":"13.0"},{"v":18,"d":"18.0"},4.8,5.8]
["FHW0630-R82M-G/B",0.82,{"v":12,"d":"12.0"},{"v":16,"d":"16.0"},6.8,8.2]
["FHW0630-1R0M-G/B",{"v":1,"d":"1.0"},{"v":10,"d":"10.0"},{"v":15,"d":"15.0"},{"v":7,"d":"7.0"},8.6]
["FHW0630-1R5M-G/B",1.5,{"v":9,"d":"9.0"},{"v":13,"d":"13.0"},{"v":9,"d":"9.0"},{"v":12,"d":"12.0"}]
["FHW0630-2R2M-G/B",2.2,{"v":8,"d":"8.0"},{"v":10,"d":"10.0"},{"v":13,"d":"13.0"},{"v":16,"d":"16.0"}]
["FHW0630-3R3M-G/B",3.3,{"v":7,"d":"7.0"},{"v":9,"d":"9.0"},{"v":18,"d":"18.0"},{"v":22,"d":"22.0"}]
["FHW0630-4R7M-G/B",4.7,{"v":6,"d":"6.0"},{"v":8,"d":"8.0"},{"v":31,"d":"31.0"},{"v":38,"d":"38.0"}]
["FHW0630-5R6M-G/B",5.6,{"v":5,"d":"5.0"},7.5,{"v":41,"d":"41.0"},{"v":50,"d":"50.0"}]
["FHW0630-6R8M-G/B",6.8,{"v":4,"d":"4.0"},{"v":7,"d":"7.0"},{"v":45,"d":"45.0"},{"v":54,"d":"54.0"}]
["FHW0630-8R2M-G/B",8.2,3.5,{"v":6,"d":"6.0"},{"v":60,"d":"60.0"},{"v":72,"d":"72.0"}]
["FHW0630P-100M-G/B",{"v":10,"d":"10.0"},{"v":3,"d":"3.0"},{"v":5,"d":"5.0"},{"v":61,"d":"61.0"},{"v":76,"d":"76.0"}]
["FHW0630P-150M-G/B",{"v":15,"d":"15.0"},2.5,4.5,{"v":100,"d":"100.0"},{"v":130,"d":"130.0"}]
["FHW0630P-220M-G/B",{"v":22,"d":"22.0"},{"v":2,"d":"2.0"},3.5,{"v":127,"d":"127.0"},{"v":152,"d":"152.0"}]
["FHW0630P-330M-G/B",{"v":33,"d":"33.0"},1.5,{"v":3,"d":"3.0"},{"v":170,"d":"170.0"},{"v":222,"d":"222.0"}]
["FHW0630P-470M-G/B",{"v":47,"d":"47.0"},1.2,2.5,{"v":210,"d":"210.0"},{"v":290,"d":"290.0"}]
["FHW0630P-101M-G/B",{"v":100,"d":"100.0"},{"v":1,"d":"1.0"},1.7,{"v":715,"d":"715.0"},{"v":858,"d":"858.0"}]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 30%"]
["Note4：The packing quantity is 1500Pcs/ disk"]
[]
[]
[]
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"0630H系列规格","index":9,"n_rows":33,"n_cols":6,"rows_kept":33,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[20,0,20,5],[21,0,21,5],[22,0,22,5],[23,0,23,5],[24,0,24,5]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺科技有限公司"]
["SMD POWER  INDUCTORS:         FHW0630H Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
["0630H","6.6±0.2","7.4MAX","3.0MAX","1.6±0.3","3.0±0.2"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW0630-R22M-B",0.2,{"v":20,"d":"20.0"},{"v":35,"d":"35.0"},2.3,2.7]
["FHW0630-R33M-B",0.33,{"v":16,"d":"16.0"},{"v":27,"d":"27.0"},3.1,3.7]
["FHW0630-R47M-B",0.47,{"v":14,"d":"14.0"},{"v":20,"d":"20.0"},3.3,4.1]
["FHW0630-R68M-B",0.68,{"v":12,"d":"12.0"},{"v":18,"d":"18.0"},4.8,{"v":6,"d":"6.0"}]
["FHW0630-1R0M-B",1,{"v":11,"d":"11.0"},{"v":16,"d":"16.0"},8.5,{"v":10,"d":"10.0"}]
["FHW0630-1R5M-B",1.5,{"v":10,"d":"10.0"},{"v":14,"d":"14.0"},10.8,{"v":13,"d":"13.0"}]
["FHW0630-2R2M-B",2.2,{"v":8,"d":"8.0"},{"v":11,"d":"11.0"},12.7,{"v":16,"d":"16.0"}]
["FHW0630-3R3M-B",3.3,{"v":7,"d":"7.0"},{"v":10,"d":"10.0"},{"v":23,"d":"23.0"},27.6]
["FHW0630-4R7M-B",4.7,{"v":6,"d":"6.0"},{"v":9,"d":"9.0"},{"v":32,"d":"32.0"},{"v":40,"d":"40.0"}]
["FHW0630-5R6M-B",5.6,{"v":5,"d":"5.0"},{"v":8,"d":"8.0"},{"v":44,"d":"44.0"},{"v":53,"d":"53.0"}]
["FHW0630-6R8M-B",6.8,{"v":4,"d":"4.0"},{"v":7,"d":"7.0"},{"v":52,"d":"52.0"},{"v":60,"d":"60.0"}]
["FHW0630-100M-B",10,{"v":3,"d":"3.0"},{"v":5,"d":"5.0"},{"v":76,"d":"76.0"},{"v":94,"d":"94.0"}]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 30%"]
["Note4：The packing quantity is 1500Pcs/ disk"]
[]
[]
[]
[]
[null,"深圳市丰辉旺科技有限公司"]
[null,"联系电话，18503051681李生"]
[null,"官网；www.jh-dzcl.com"]

{"sheet":"0630T系列规格","index":10,"n_rows":32,"n_cols":6,"rows_kept":32,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[20,0,20,5],[21,0,21,5],[22,0,22,4],[23,0,23,4],[24,0,24,4]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺科技有限公司"]
[" SMD POWER  INDUCTORS:       FHW0630T Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
["0630T","6.6±0.2","7.4MAX","3.0MAX","1.6±0.3","3.0±0.2"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW0630-R33M-G/B",0.33,{"v":18,"d":"18.0"},{"v":32,"d":"32.0"},2.9,3.5]
["FHW0630-R47M-G/B",0.47,{"v":15,"d":"15.0"},{"v":26,"d":"26.0"},{"v":3,"d":"3.0"},4.2]
["FHW0630-R68M-G/B",0.68,{"v":14,"d":"14.0"},{"v":25,"d":"25.0"},4.8,{"v":6,"d":"6.0"}]
["FHW0630-R82M-G/B",0.82,{"v":13,"d":"13.0"},{"v":24,"d":"24.0"},7.4,8.5]
["FHW0630-1R0M-G/B",{"v":1,"d":"1.0"},{"v":12,"d":"12.0"},{"v":22,"d":"22.0"},8.5,{"v":10,"d":"10.0"}]
["FHW0630TP-1R5M-G/B",1.5,{"v":10,"d":"10.0"},{"v":18,"d":"18.0"},9.3,{"v":12,"d":"12.0"}]
["FHW0630TP-2R2M-G/B",2.2,{"v":8,"d":"8.0"},{"v":14,"d":"14.0"},{"v":15,"d":"15.0"},{"v":20,"d":"20.0"}]
["FHW0630TP-3R3M-G/B",3.3,6.5,{"v":13,"d":"13.0"},{"v":22,"d":"22.0"},{"v":30,"d":"30.0"}]
["FHW0630TP-4R7M-G/B",4.7,{"v":6,"d":"6.0"},{"v":10,"d":"10.0"},{"v":30,"d":"30.0"},{"v":44,"d":"44.0"}]
["FHW0630TP-5R6M-G/B",5.6,{"v":5,"d":"5.0"},{"v":9,"d":"9.0"},{"v":44,"d":"44.0"},{"v":50,"d":"50.0"}]
["FHW0630TP-6R8M-G/B",6.8,4.5,{"v":8,"d":"8.0"},{"v":50,"d":"50.0"},{"v":60,"d":"60.0"}]
["FHW0630TP-100M-G/B",10,3.5,{"v":7,"d":"7.0"},{"v":70,"d":"70.0"},{"v":96,"d":"96.0"}]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 25%"]
["Note4：The packing quantity is 1500Pcs/ disk"]
[]
[]
[]
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"0630TF系系列规格","index":11,"n_rows":33,"n_cols":6,"rows_kept":33,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[19,0,19,5],[20,0,20,5],[21,0,21,4],[22,0,22,4],[23,0,23,4],[24,0,24,2]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺科技有限公司"]
[" SMD POWER  INDUCTORS:      FHW0630 Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
["0630T","6.6±0.2","7.4MAX","3.0MAX","1.6±0.3","3.0±0.2"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW0630-R10M-C/B",0.1,32.5,{"v":60,"d":"60.0"},1.5,1.7]
["FHW0630-R56M-C/B",0.56,{"v":15,"d":"15.0"},{"v":25,"d":"25.0"},{"v":5,"d":"5.0"},{"v":6,"d":"6.0"}]
["FHW0630-R82M-C/B",0.82,{"v":12,"d":"12.0"},{"v":20,"d":"20.0"},8.5,{"v":10,"d":"10.0"}]
["FHW0630-1R0M-C/B",{"v":1,"d":"1.0"},{"v":11,"d":"11.0"},{"v":20,"d":"20.0"},8.5,{"v":10,"d":"10.0"}]
["FHW0630-1R5M-C/B",1.5,{"v":9,"d":"9.0"},{"v":18,"d":"18.0"},{"v":10,"d":"10.0"},{"v":15,"d":"15.0"}]
["FHW0630-2R2M-C/B",2.2,{"v":6,"d":"6.0"},{"v":12,"d":"12.0"},{"v":14,"d":"14.0"},{"v":17,"d":"17.0"}]
["FHW0630-3R3M-C/B",3.3,{"v":6,"d":"6.0"},{"v":11,"d":"11.0"},{"v":22,"d":"22.0"},26.5]
["FHW0630-4R7M-C/B",4.7,{"v":5,"d":"5.0"},{"v":9,"d":"9.0"},{"v":35,"d":"35.0"},{"v":42,"d":"42.0"}]
["FHW0630-6R8M-C/B",5.6,4.5,{"v":8,"d":"8.0"},{"v":47,"d":"47.0"},{"v":60,"d":"60.0"}]
["FHW0630-8R2M-C/B",6.8,4.5,7.5,{"v":61,"d":"61.0"},{"v":73,"d":"73.0"}]
["FHW0630-100M-C/B",10,{"v":4,"d":"4.0"},{"v":7,"d":"7.0"},{"v":78,"d":"78.0"},{"v":94,"d":"94.0"}]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 30%"]
["Note4：The packing quantity is 1500Pcs/ disk"]
[]
[]
[]
[]
[]
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"0640系列规格","index":12,"n_rows":34,"n_cols":10,"rows_kept":34,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[21,0,21,5],[22,0,22,5],[23,0,23,5],[24,0,24,5],[25,0,25,5]],"flags":["formulas_cached_only"]}
[" 深圳市丰辉旺科技有限公司"]
["SMD POWER  INDUCTORS:          FHW0640 Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
[640,"6.6±0.2","7.6MAX","4.0MAX","1.6±0.3","3.0±0.2"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW0640-R47M-G/B",0.47,{"v":15,"d":"15.0"},{"v":26,"d":"26.0"},{"v":3,"d":"3.0"},3.6]
["FHW0640-R68M-G/B",0.68,{"v":10,"d":"10.0"},{"v":18,"d":"18.0"},4.8,5.8,{"$nulls":3},1]
["FHW0640-1R0M-G/B",{"v":1,"d":"1.0"},{"v":9,"d":"9.0"},{"v":17,"d":"17.0"},5.5,6.6]
["FHW0640-1R5M-G/B",1.5,{"v":8,"d":"8.0"},{"v":13,"d":"13.0"},7,10.8]
["FHW0640-2R2M-G/B",2.2,{"v":7,"d":"7.0"},{"v":12,"d":"12.0"},{"v":10,"d":"10.0"},{"v":13,"d":"13.0"}]
["FHW0640-3R3M-G/B",3.3,6.5,{"v":11,"d":"11.0"},13.5,{"v":18,"d":"18.0"}]
["FHW0640-4R7M-G/B",4.7,{"v":6,"d":"6.0"},{"v":9,"d":"9.0"},{"v":20,"d":"20.0"},{"v":24,"d":"24.0"}]
["FHW0640-6R8M-G/B",6.8,{"v":5,"d":"5.0"},{"v":8,"d":"8.0"},{"v":41,"d":"41.0"},{"v":49,"d":"49.0"}]
["FHW0640-8R2M-G/B",8.2,{"v":4,"d":"4.0"},{"v":7,"d":"7.0"},{"v":58,"d":"58.0"},{"v":70,"d":"70.0"}]
["FHW0640-100M-G/B",{"v":10,"d":"10.0"},3.5,6.5,{"v":58,"d":"58.0"},{"v":70,"d":"70.0"}]
["FHW0640-150M-G/B",15,{"v":3,"d":"3.0"},5.5,{"v":64,"d":"64.0"},{"v":77,"d":"77.0"}]
["FHW0640-220M-G/B",{"v":22,"d":"22.0"},2.5,{"v":4,"d":"4.0"},{"v":98,"d":"98.0"},{"v":117,"d":"117.0"}]
["FHW0640-330M-G/B",{"v":33,"d":"33.0"},{"v":2,"d":"2.0"},3.5,{"v":163,"d":"163.0"},{"v":196,"d":"196.0"}]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 30%"]
["Note4：The packing quantity is 1000Pcs/ disk"]
[]
[]
[]
[]
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"0650系列规格","index":13,"n_rows":37,"n_cols":6,"rows_kept":37,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[25,0,25,5],[26,0,26,5],[27,0,27,5],[28,0,28,5],[29,0,29,5]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺科技有限公司"]
["SMD POWER  INDUCTORS:          FHW0650 Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
[650,"6.6±0.2","7.6MAX","5.0MAX","1.6±0.3","3.0±0.2"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW-0650-R47M-G/B",0.47,{"v":14,"d":"14.0"},{"v":24,"d":"24.0"},3.1,{"v":4,"d":"4.0"}]
["FHW-0650-R68M-G/B",0.68,{"v":11,"d":"11.0"},{"v":20,"d":"20.0"},4.5,5.4]
["FHW-0650-R82M-G/B",0.82,{"v":10,"d":"10.0"},{"v":19,"d":"19.0"},{"v":6,"d":"6.0"},7.2]
["FHW-0650-1R0M-G/B",{"v":1,"d":"1.0"},{"v":9,"d":"9.0"},{"v":18,"d":"18.0"},{"v":6,"d":"6.0"},7.2]
["FHW-0650-1R5M-G/B",1.5,8.5,{"v":15,"d":"15.0"},{"v":7,"d":"7.0"},8.5]
["FHW-0650-2R2M-G/B",2.2,{"v":8,"d":"8.0"},{"v":14,"d":"14.0"},10.4,12.5]
["FHW-0650-3R3M-G/B",3.3,{"v":7,"d":"7.0"},{"v":11,"d":"11.0"},{"v":13,"d":"13.0"},{"v":16,"d":"16.0"}]
["FHW-0650-4R7M-G/B",4.7,{"v":6,"d":"6.0"},{"v":10,"d":"10.0"},{"v":17,"d":"17.0"},{"v":20,"d":"20.0"}]
["FHW-0650-6R8M-G/B",6.8,{"v":5,"d":"5.0"},{"v":9,"d":"9.0"},{"v":22,"d":"22.0"},26.4]
["FHW-0650-8R2M-G/B",8.2,4.5,8.5,{"v":33,"d":"33.0"},{"v":45,"d":"45.0"}]
["FHW-0650-100M-G/B",{"v":10,"d":"10.0"},{"v":4,"d":"4.0"},{"v":8,"d":"8.0"},{"v":37,"d":"37.0"},{"v":46,"d":"46.0"}]
["FHW-0650-150M-G/B",{"v":15,"d":"15.0"},3.5,{"v":6,"d":"6.0"},{"v":54,"d":"54.0"},{"v":65,"d":"65.0"}]
["FHW-0650-220M-G/B",{"v":22,"d":"22.0"},{"v":3,"d":"3.0"},{"v":5,"d":"5.0"},{"v":80,"d":"80.0"},{"v":105,"d":"105.0"}]
["FHW0650-330M-G/B",{"v":33,"d":"33.0"},2.5,4.5,{"v":120,"d":"120.0"},{"v":144,"d":"144.0"}]
["FHW-0650-470M-G/B",{"v":47,"d":"47.0"},1.5,2.5,{"v":170,"d":"170.0"},{"v":200,"d":"200.0"}]
["FHW-0650-560M-G/B",{"v":56,"d":"56.0"},1.4,2.4,{"v":202,"d":"202.0"},{"v":242,"d":"242.0"}]
["FHW-0650-101M-G/B",100,{"v":1,"d":"1.0"},{"v":2,"d":"2.0"},{"v":265,"d":"265.0"},{"v":320,"d":"320.0"}]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 30%"]
["Note4：The packing quantity is 1000Pcs/ disk"]
[]
[]
[]
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"0850系列规格","index":14,"n_rows":42,"n_cols":10,"rows_kept":42,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[28,0,28,5],[29,0,29,5],[30,0,30,5],[31,0,31,5],[32,0,32,5]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺科技有限公司"]
["         FHWHJ0850 "]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
[850,"8.0±0.3","9.2MAX","5.0MAX","1.8±0.3","3.0±0.2"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHWHJ0850-R82MB",0.82,{"v":16,"d":"16.0"},{"v":24,"d":"24.0"},{"v":4,"d":"4.0"},4.8]
["FHWHJ0850-1R0MB",1,{"v":14,"d":"14.0"},{"v":21,"d":"21.0"},4.7,5.6]
["FHWHJ0850-2R2MB",2.2,{"v":11,"d":"11.0"},{"v":18,"d":"18.0"},7.5,{"v":9,"d":"9.0"}]
["FHWHJ0850-3R3MB",3.3,{"v":10,"d":"10.0"},{"v":15,"d":"15.0"},{"v":11,"d":"11.0"},{"v":13,"d":"13.0"}]
["FHWHJ0850-4R7MB",4.7,{"v":8,"d":"8.0"},{"v":14,"d":"14.0"},{"v":16,"d":"16.0"},{"v":20,"d":"20.0"}]
["FHWHJ0850-6R8MB",6.8,{"v":6,"d":"6.0"},{"v":11,"d":"11.0"},{"v":20,"d":"20.0"},{"v":24,"d":"24.0"}]
["FHWHJ0850-100MB",{"v":10,"d":"10.0"},{"v":5,"d":"5.0"},{"v":10,"d":"10.0"},{"v":30,"d":"30.0"},{"v":36,"d":"36.0"}]
["FHWHJ0850-150MB",{"v":15,"d":"15.0"},{"v":4,"d":"4.0"},7.5,{"v":46,"d":"46.0"},{"v":55,"d":"55.0"}]
["FHWHJ0850-220MB",22,3.5,{"v":7,"d":"7.0"},{"v":78,"d":"78.0"},{"v":94,"d":"94.0"},null,null,"A"]
["FHWHJ0850-330MB",33,{"v":3,"d":"3.0"},{"v":6,"d":"6.0"},{"v":125,"d":"125.0"},{"v":150,"d":"150.0"}]
["FHWHJ0850-470MB",47,2.5,{"v":4,"d":"4.0"},{"v":160,"d":"160.0"},{"v":192,"d":"192.0"}]
["FHWHJ0850-560MB",56,{"v":2,"d":"2.0"},3.5,{"v":170,"d":"170.0"},{"v":205,"d":"205.0"}]
[{"$nulls":6},188,233,"3A","1.5A"]
[{"$nulls":6},272,326,"2A","1.2A"]
[]
[]
[]
[]
["FHWHJ0850-680MB",68,1.5,{"v":3,"d":"3.0"},{"v":188,"d":"188.0"},{"v":233,"d":"233.0"}]
["FHWHJ0850-101M-G/B",100,1.2,{"v":2,"d":"2.0"},{"v":272,"d":"272.0"},{"v":326,"d":"326.0"}]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 30%"]
["Note4:The packing quantity is 1000Pcs/ disk"]
[]
[]
[]
[]
[]
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"1040系列规格","index":15,"n_rows":41,"n_cols":6,"rows_kept":41,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[28,0,28,5],[29,0,29,5],[30,0,30,5],[31,0,31,5],[32,0,32,5],[33,0,33,5]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺科技有限公司"]
["SMD POWER INDUCTORS:       FHW1040/45 Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
["1040/45","10.3±0.3","10.5±1.0","4.0MAX/4.5MAX","2.0±0.5","3.0±0.3"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW1040-R22M-G/B",0.22,{"v":30,"d":"30.0"},{"v":54,"d":"54.0"},0.8,{"v":1,"d":"1.0"}]
["FHW1040-R36M-G/B",0.36,{"v":25,"d":"25.0"},{"v":45,"d":"45.0"},1.1,1.4]
["FHW1040-R47M-G/B",0.47,{"v":20,"d":"20.0"},{"v":35,"d":"35.0"},1.2,1.5]
["FHW1040-R56M-G/B",0.56,{"v":18,"d":"18.0"},{"v":34,"d":"34.0"},1.6,1.9]
["FHW1040-R68M-G/B",0.68,{"v":17,"d":"17.0"},{"v":32,"d":"32.0"},1.6,1.9]
["FHW1040-R82M-G/B",0.82,{"v":16,"d":"16.0"},{"v":28,"d":"28.0"},1.8,2.4]
["FHW1040-1R0M-G/B",{"v":1,"d":"1.0"},{"v":15,"d":"15.0"},{"v":23,"d":"23.0"},2.1,2.5]
["FHW1040-1R5M-G/B",1.5,{"v":14,"d":"14.0"},{"v":22,"d":"22.0"},4.4,5.3]
["FHW1040-2R2M-G/B",2.2,{"v":11,"d":"11.0"},{"v":18,"d":"18.0"},{"v":6.4,"d":"6.40"},{"v":7,"d":"7.0"}]
["FHW1040-3R3M-G/B",3.3,{"v":10,"d":"10.0"},{"v":17,"d":"17.0"},{"v":9,"d":"9.0"},11.5]
["FHW1040-4R7M-G/B",4.7,{"v":8,"d":"8.0"},{"v":13,"d":"13.0"},{"v":12,"d":"12.0"},{"v":15,"d":"15.0"}]
["FHW1040-5R6M-G/B",5.6,{"v":7,"d":"7.0"},{"v":12,"d":"12.0"},{"v":16,"d":"16.0"},19.2]
["FHW1040-6R8M-G/B",6.8,{"v":6,"d":"6.0"},{"v":11,"d":"11.0"},17.5,{"v":22,"d":"22.0"}]
["FHW1040-8R2M-G/B",8.2,5.5,{"v":10,"d":"10.0"},{"v":27,"d":"27.0"},{"v":32,"d":"32.0"}]
["FHW1040-100M-G/B",{"v":10,"d":"10.0"},{"v":5,"d":"5.0"},{"v":9,"d":"9.0"},{"v":31,"d":"31.0"},{"v":40,"d":"40.0"}]
["FHW1045-150M-G/B",{"v":15,"d":"15.0"},{"v":4,"d":"4.0"},{"v":8,"d":"8.0"},{"v":37,"d":"37.0"},{"v":60,"d":"60.0"}]
["FHW1045-220M-G/B",{"v":22,"d":"22.0"},{"v":4,"d":"4.0"},{"v":6,"d":"6.0"},{"v":54,"d":"54.0"},{"v":72,"d":"72.0"}]
["FHW1045-330M-G/B",{"v":33,"d":"33.0"},3.5,{"v":5,"d":"5.0"},{"v":82,"d":"82.0"},{"v":105,"d":"105.0"}]
["FHW1045-470M-G/B",{"v":47,"d":"47.0"},2.5,4.5,{"v":128,"d":"128.0"},{"v":158,"d":"158.0"}]
["FHW1045Y-101M-G/B",100,{"v":2,"d":"2.0"},3.5,{"v":237,"d":"237.0"},{"v":290,"d":"290.0"}]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 30%"]
["Note4：The packing quantity of the 1040 series is 1000Pcs/ disk, and the number of packaging in 1045 is 800Pcs/ disk."]
[]
[]
[]
[]
[null,"深圳市丰辉旺科技有限公司"]
[null,"联系电话，18503051681李生"]
[null,"官网；www.jh-dzcl.com"]

{"sheet":"1040T系列规格","index":16,"n_rows":35,"n_cols":6,"rows_kept":35,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[22,0,22,5],[23,0,23,5],[24,0,24,5],[25,0,25,5],[26,0,26,5],[27,0,27,5]],"flags":["formulas_cached_only"]}
[" 深圳市丰辉旺科技有限公司"]
["SMD POWER INDUCTORS:       FHW1040 Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
[1040,"10.3±0.3","10.5±1.0","4.0MAX/4.5MAX","2.0±0.5","3.0±0.3"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW1040-R22M-G/B",0.22,"35A","65A",0.6,{"v":0.95,"d":"1.0"}]
["FHW1040-R33M-G/B",0.33,"32A","63A",1.1,1.4]
["FHW1040-R36M-G/B",0.36,"30A","60A",1.1,1.4]
["FHW1040-R47M-G/B",0.47,"28A","55A",1.4,{"v":1.68,"d":"1.7"}]
["FHW1040-R56M-G/B",0.56,"27.5A","49A",1.7,1.8]
["FHW1040-R68M-G/B",0.68,"25A","45A",2.2,2.4]
["FHW1040-1R0M-G/B",{"v":1,"d":"1.0"},"18A","32A",2.6,3.7]
["FHW1040-1R5M-G/B",1.5,"15A","27.5A",{"v":5,"d":"5.0"},5.8]
["FHW1040-2R2M-G/B",2.2,"12A","27A",5.7,{"v":10,"d":"10.0"}]
["FHW1040-3R3M-G/B",3.3,"11A","20A",10.5,{"v":12,"d":"12.0"}]
["FHW1040-4R7M-G/B",4.7,"10A","17A",13.5,16.5]
["FHW1040-100M-G/B",10,"8A","12A",{"v":31,"d":"31.0"},{"v":40,"d":"40.0"}]
["FHW1040-150M-G/B",15,"7A","11A",{"v":53,"d":"53.0"},{"v":70,"d":"70.0"}]
["FHW1040-220M-G/B",22,"4A","7A",{"v":59,"d":"59.0"},{"v":70,"d":"70.0"}]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 25%"]
["Note4：The packing quantity of the 1040 series is 1000Pcs/ disk"]
[]
[]
[]
[]
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"1050系列规格","index":17,"n_rows":49,"n_cols":6,"rows_kept":49,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[32,0,32,5],[33,0,33,5],[34,0,34,5],[35,0,35,5],[36,0,36,5]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺科技有限公司"]
["         FHW-1050 "]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
[1050,"10.3±0.3","10.5±1.0","5.0MAX","2.0±0.5","3.0±0.3"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW-1045-100MB",{"v":10,"d":"10.0"},0.1,11.5,6.8,{"v":38,"d":"38.0"}]
["FHW-1045-150MB",{"v":15,"d":"15.0"},{"v":5,"d":"5.0"},{"v":9,"d":"9.0"},{"v":48,"d":"48.0"},{"v":55,"d":"55.0"}]
["FHW-1045-220MB",{"v":22,"d":"22.0"},4.5,{"v":8,"d":"8.0"},{"v":50,"d":"50.0"},{"v":58,"d":"58.0"}]
["FHW-1045-330MB",{"v":33,"d":"33.0"},3.5,6.5,{"v":75,"d":"75.0"},{"v":90,"d":"90.0"}]
["FHW-1050-470MB",{"v":47,"d":"47.0"},{"v":3,"d":"3.0"},{"v":5,"d":"5.0"},{"v":110,"d":"110.0"},{"v":130,"d":"130.0"}]
["FHW-1050Y-R82MB",0.82,{"v":18,"d":"18.0"},{"v":34,"d":"34.0"},1.8,2.2]
["FHW-1050Y-1R0MB",{"v":1,"d":"1.0"},{"v":16,"d":"16.0"},{"v":28,"d":"28.0"},2.1,2.5]
["FHW-1050Y-1R2MB",1.2,{"v":15,"d":"15.0"},{"v":26,"d":"26.0"},2.3,2.8]
["FHW-1050Y-1R5MB",1.5,{"v":13,"d":"13.0"},{"v":21,"d":"21.0"},2.6,3.1]
["FHW-1050Y-2R2MB",2.2,{"v":11,"d":"11.0"},{"v":20,"d":"20.0"},5.2,{"v":7,"d":"7.0"}]
["FHW-1050Y-3R3MB",3.3,{"v":10,"d":"10.0"},{"v":16,"d":"16.0"},{"v":6,"d":"6.0"},7.8]
["FHW-1050Y-4R7MB",4.7,{"v":9,"d":"9.0"},{"v":15,"d":"15.0"},10.8,{"v":12,"d":"12.0"}]
["FHW-1050Y-5R6MB",5.6,{"v":8,"d":"8.0"},{"v":14,"d":"14.0"},13.5,{"v":16,"d":"16.0"}]
["FHW-1050Y-6R8MB",6.8,7.5,{"v":13,"d":"13.0"},13.5,{"v":16,"d":"16.0"}]
["FHW-1050Y-8R2MB",8.2,{"v":7,"d":"7.0"},12.5,{"v":22,"d":"22.0"},{"v":25,"d":"25.0"}]
["FHW-1050Y-100MB",{"v":10,"d":"10.0"},{"v":6,"d":"6.0"},{"v":12,"d":"12.0"},{"v":23,"d":"23.0"},{"v":28,"d":"28.0"}]
["FHW-1050Y-150MB",{"v":15,"d":"15.0"},{"v":5,"d":"5.0"},{"v":10,"d":"10.0"},{"v":33,"d":"33.0"},{"v":42,"d":"42.0"}]
["FHW-1050Y-220MB",{"v":22,"d":"22.0"},4.5,{"v":8,"d":"8.0"},{"v":58,"d":"58.0"},{"v":70,"d":"70.0"}]
["FHW-1050Y-330MB",{"v":33,"d":"33.0"},{"v":4,"d":"4.0"},{"v":6,"d":"6.0"},{"v":85,"d":"85.0"},{"v":105,"d":"105.0"}]
["FHW-1050Y-470MB",{"v":47,"d":"47.0"},3.5,5.5,{"v":127,"d":"127.0"},{"v":152,"d":"152.0"}]
["FHW-1050Y-680MB",{"v":68,"d":"68.0"},{"v":3,"d":"3.0"},{"v":5,"d":"5.0"},{"v":198,"d":"198.0"},{"v":258,"d":"258.0"}]
["FHW-1050Y-820MB",{"v":82,"d":"82.0"},2.5,4.5,{"v":220,"d":"220.0"},{"v":264,"d":"264.0"}]
["FHW-1050Y-101MB",{"v":100,"d":"100.0"},{"v":2,"d":"2.0"},{"v":4,"d":"4.0"},{"v":230,"d":"230.0"},{"v":279,"d":"279.0"}]
["FHW-1050Y-151MB",{"v":150,"d":"150.0"},1.5,{"v":3,"d":"3.0"},{"v":412,"d":"412.0"},{"v":495,"d":"495.0"}]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 30%"]
["Note4：The packing quantity is 800Pcs/ disk"]
{"$rows_empty":8}
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"1240系列规格","index":18,"n_rows":37,"n_cols":6,"rows_kept":37,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[23,0,23,5],[24,0,24,5],[25,0,25,5],[26,0,26,5],[27,0,27,5]],"flags":["formulas_cached_only"]}
["深圳丰辉旺电子科技有限公司"]
["SMD POWER INDUCTORS:             FHW- 1240 Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
[1240,"12.8±0.5","13.2±1.0","4.0MAX","2.5±0.5","3.8±0.3"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW-1240Y-R22M-G/B",0.22,{"v":35,"d":"35.0"},{"v":55,"d":"55.0"},0.7,0.9]
["FHW-1240Y-R33M-G/B",0.33,{"v":30,"d":"30.0"},{"v":50,"d":"50.0"},0.8,1.5]
["FHW-1240Y-R47M-G/B",0.47,{"v":25,"d":"25.0"},{"v":45,"d":"45.0"},1.3,1.6]
["FHW-1240Y-R56M-G/B",0.56,{"v":22,"d":"22.0"},{"v":42,"d":"42.0"},1.5,1.8]
["FHW-1240Y-R68M-G/B",0.68,{"v":20,"d":"20.0"},{"v":40,"d":"40.0"},1.7,{"v":2,"d":"2.0"}]
["FHW-1240Y-1R0M-G/B",{"v":1,"d":"1.0"},{"v":18,"d":"18.0"},{"v":38,"d":"38.0"},2.9,3.5]
["FHW-1240Y-1R5M-G/B",1.5,{"v":15,"d":"15.0"},{"v":30,"d":"30.0"},4.4,5.3]
["FHW-1240Y-2R2M-G/B",2.2,{"v":12,"d":"12.0"},{"v":20,"d":"20.0"},{"v":5,"d":"5.0"},6.5]
["FHW-1240Y-3R3M-G/B",3.3,{"v":11,"d":"11.0"},{"v":18,"d":"18.0"},6.7,{"v":8,"d":"8.0"}]
["FHW-1240Y-4R7M-G/B",4.7,{"v":10,"d":"10.0"},{"v":16,"d":"16.0"},14.5,17.5]
["FHW-1240Y-5R6M-G/B",5.6,{"v":8,"d":"8.0"},{"v":15,"d":"15.0"},14.5,17.5]
["FHW-1240Y-6R8M-G/B",6.8,{"v":6,"d":"6.0"},{"v":11,"d":"11.0"},{"v":19,"d":"19.0"},{"v":30,"d":"30.0"}]
["FHW-1240Y-100M-G/B",10,{"v":5,"d":"5.0"},{"v":8,"d":"8.0"},{"v":27,"d":"27.0"},{"v":33,"d":"33.0"}]
["FHW-1240Y-220M-G/B",{"v":22,"d":"22.0"},{"v":4,"d":"4.0"},{"v":7,"d":"7.0"},{"v":49,"d":"49.0"},{"v":58,"d":"58.0"}]
[]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 30%"]
["Note4：The packing quantity is 500Pcs/ disk"]
[]
[]
[]
[]
[]
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"1250系列规格","index":19,"n_rows":41,"n_cols":6,"rows_kept":41,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[28,0,28,5],[29,0,29,5],[30,0,30,5],[31,0,31,5],[32,0,32,5]],"flags":["formulas_cached_only"]}
["深圳市电子科技有限公司"]
["SMD POWER INDUCTORS:              FHW-1250 Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
[1250,"12.8±0.5","13.2±1.0","5.0MAX","2.5±0.5","3.8±0.3"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW-1250Y-R36M-G/B",0.36,{"v":40,"d":"40.0"},{"v":60,"d":"60.0"},1,1.2]
["FHW-1250Y-R47M-G/B",0.47,{"v":25,"d":"25.0"},{"v":45,"d":"45.0"},{"v":1,"d":"1.0"},1.2]
["FHW-1250Y-R56M-G/B",0.56,{"v":24,"d":"24.0"},{"v":40,"d":"40.0"},{"v":1,"d":"1.0"},1.2]
["FHW-1250Y-R68M-G/B",0.68,{"v":23,"d":"23.0"},{"v":38,"d":"38.0"},1.2,1.6]
["FHW-1250Y-R82M-G/B",0.82,{"v":22,"d":"22.0"},{"v":36,"d":"36.0"},1.7,2.2]
["FHW-1250Y-1R0M-G/B",{"v":1,"d":"1.0"},{"v":20,"d":"20.0"},{"v":35,"d":"35.0"},2.1,2.5]
["FHW-1250Y-1R2M-G/B",1.2,{"v":16,"d":"16.0"},{"v":32,"d":"32.0"},2.1,2.6]
["FHW-1250Y-1R5M-G/B",1.5,{"v":15,"d":"15.0"},{"v":30,"d":"30.0"},2.6,3.1]
["FHW-1250Y-2R2M-G/B",2.2,{"v":14,"d":"14.0"},{"v":26,"d":"26.0"},{"v":5,"d":"5.0"},{"v":6,"d":"6.0"}]
["FHW-1250Y-3R3M-G/B",3.3,{"v":13,"d":"13.0"},{"v":24,"d":"24.0"},6.3,7.6]
["FHW-1250Y-4R7M-G/B",4.7,{"v":12,"d":"12.0"},{"v":18,"d":"18.0"},7.5,{"v":9,"d":"9.0"}]
["FHW-1250Y-5R6M-G/B",5.6,{"v":9,"d":"9.0"},{"v":15,"d":"15.0"},7.5,10.5]
["FHW-1250Y-6R8M-G/B",6.8,{"v":8,"d":"8.0"},{"v":13,"d":"13.0"},{"v":12,"d":"12.0"},14.4]
["FHW-1250Y-8R2M-G/B",8.2,7.5,{"v":12,"d":"12.0"},{"v":18,"d":"18.0"},{"v":22,"d":"22.0"}]
["FHW-1250Y-100M-G/B",{"v":10,"d":"10.0"},{"v":7,"d":"7.0"},{"v":11,"d":"11.0"},19.5,{"v":24,"d":"24.0"}]
["FHW-1250Y-150M-G/B",15,{"v":5,"d":"5.0"},{"v":9,"d":"9.0"},{"v":26,"d":"26.0"},31.2]
["FHW-1250Y-220M-G/B",22,{"v":4,"d":"4.0"},{"v":7,"d":"7.0"},{"v":29,"d":"29.0"},35]
["FHW-1250Y-330M-G/B",33,{"v":3,"d":"3.0"},{"v":6,"d":"6.0"},{"v":52,"d":"52.0"},63]
["FHW-1250Y-470M-G/B",47,2.5,{"v":5,"d":"5.0"},{"v":85,"d":"85.0"},102]
[]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 30%"]
["Note4：The packing quantity is 500Pcs/ disk"]
[]
[]
[]
[]
[null,"深圳市丰辉旺科技有限公司"]
[null,"联系电话，18503051681李生"]
[null,"官网；www.jh-dzcl.com"]

{"sheet":"1260系列规格 ","index":20,"n_rows":42,"n_cols":6,"rows_kept":42,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[26,0,26,5],[27,0,27,5],[28,0,28,5],[29,0,29,5],[30,0,30,5],[31,0,31,5]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺电子科技有限公司"]
["SMD POWER INDUCTORS:      1260/65 Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
["1260/65","12.8±0.5","13.2±1.0","6.0/6.5MAX","2.5±0.5","3.8±0.3"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW-1260Y-R68M-G/B",0.68,{"v":30,"d":"30.0"},{"v":45,"d":"45.0"},1.1,1.8]
["FHW-1260Y-R82M-G/B",0.82,{"v":25,"d":"25.0"},{"v":42,"d":"42.0"},1.5,2.4]
["FHW-1260Y-1R0M-G/B",1,{"v":24,"d":"24.0"},{"v":40,"d":"40.0"},2.2,2.6]
["FHW-1260Y-1R5M-G/B",1.5,{"v":18,"d":"18.0"},{"v":30,"d":"30.0"},2.1,4.1]
["FHW-1260Y-2R2M-G/B",2.2,{"v":16,"d":"16.0"},{"v":28,"d":"28.0"},{"v":5,"d":"5.0"},{"v":6,"d":"6.0"}]
["FHW-1260Y-3R3M-G/B",3.3,{"v":15,"d":"15.0"},{"v":26,"d":"26.0"},5.4,6.5]
["FHW-1260Y-4R7M-G/B",4.7,{"v":14,"d":"14.0"},{"v":24,"d":"24.0"},7.5,{"v":9,"d":"9.0"}]
["FHW-1260Y-5R6M-G/B",5.6,{"v":12,"d":"12.0"},{"v":18,"d":"18.0"},7.7,{"v":10,"d":"10.0"}]
["FHW-1260Y-6R8M-G/B",6.8,{"v":10,"d":"10.0"},{"v":16,"d":"16.0"},8.4,{"v":10,"d":"10.0"}]
["FHW-1260Y-8R2M-G/B",8.2,9,15,10.9,13]
["FHW-1265Y-100M-G/B",{"v":10,"d":"10.0"},{"v":8,"d":"8.0"},{"v":13,"d":"13.0"},11.4,{"v":15,"d":"15.0"}]
["FHW-1265Y-150M-G/B",15,6.5,12,18,22]
["FHW-1265Y-220M-G/B",{"v":22,"d":"22.0"},{"v":6,"d":"6.0"},{"v":10,"d":"10.0"},{"v":30,"d":"30.0"},{"v":36,"d":"36.0"}]
["FHW-1265Y-330M-G/B",33,5,9,38,53]
["FHW-1265Y-470M-G/B",{"v":47,"d":"47.0"},{"v":4,"d":"4.0"},{"v":6,"d":"6.0"},{"v":50,"d":"50.0"},{"v":96,"d":"96.0"}]
["FHW-1265Y-680M-G/B",68,3,5.5,95.5,115]
["FHW-1265Y-820M-G/B",{"v":82,"d":"82.0"},2.5,4.5,105,{"v":126,"d":"126.0"}]
["FHW-1265Y-101M-G/B",100,2,4,98,147]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 30%"]
["Note4：The packing quantity of 1260 is 500Pcs/ disk, and the quantity of 1265 is 400Pcs/ disk."]
{"$rows_empty":7}
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"1770系列规格","index":21,"n_rows":41,"n_cols":6,"rows_kept":41,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[22,0,22,5],[23,0,23,5],[24,0,24,5],[25,0,25,5],[26,0,26,5],[27,0,27,5]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺电子科技有限公司"]
["SMD POWER INDUCTORS:        FHW-1770 Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
[1770,"17.15MAX","17.5±1.0","7.0MAX","2.0±0.5","11.94±0.3"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW-1770Y-2R2M-G/B",2.2,{"v":28,"d":"28.0"},{"v":40,"d":"40.0"},2.3,2.7]
["FHW-1770Y-4R7M-G/B",4.7,{"v":16,"d":"16.0"},{"v":26,"d":"26.0"},3.9,4.7]
["FHW-1770Y-6R8M-G/B",6.8,{"v":13,"d":"13.0"},{"v":23,"d":"23.0"},5.6,6.9]
["FHW-1770Y-8R2M-G/B",8.2,{"v":12,"d":"12.0"},{"v":22,"d":"22.0"},{"v":7,"d":"7.0"},8.4]
["FHW-1770Y-100M-G/B",{"v":10,"d":"10.0"},{"v":10,"d":"10.0"},{"v":18,"d":"18.0"},{"v":6.95,"d":"7.0"},8.5]
["FHW-1770Y-150M-G/B",{"v":15,"d":"15.0"},{"v":9,"d":"9.0"},{"v":17,"d":"17.0"},17.7,{"v":22,"d":"22.0"}]
["FHW-1770Y-220M-G/B",{"v":22,"d":"22.0"},{"v":8,"d":"8.0"},{"v":15,"d":"15.0"},{"v":20,"d":"20.0"},{"v":25,"d":"25.0"}]
["FHW-1770Y-330M-G/B",{"v":33,"d":"33.0"},6.5,{"v":10,"d":"10.0"},{"v":27,"d":"27.0"},{"v":35,"d":"35.0"}]
["FHW-1770Y-470M-G/B",{"v":47,"d":"47.0"},{"v":6,"d":"6.0"},{"v":9,"d":"9.0"},{"v":39,"d":"39.0"},{"v":47,"d":"47.0"}]
["FHW-1770Y-680M-G/B",{"v":68,"d":"68.0"},{"v":5,"d":"5.0"},8.5,{"v":67,"d":"67.0"},{"v":80,"d":"80.0"}]
["FHW-1770Y-820M-G/B",{"v":82,"d":"82.0"},4.5,{"v":8,"d":"8.0"},{"v":86,"d":"86.0"},{"v":100,"d":"100.0"}]
["FHW-1770Y-101M-G/B",{"v":100,"d":"100.0"},{"v":4,"d":"4.0"},{"v":7,"d":"7.0"},{"v":95,"d":"95.0"},{"v":125,"d":"125.0"}]
["FHW-1770Y-151M-G/B",{"v":150,"d":"150.0"},{"v":3,"d":"3.0"},{"v":5,"d":"5.0"},{"v":135,"d":"135.0"},{"v":162,"d":"162.0"}]
["FHW-1770Y-351M-G/B",{"v":350,"d":"350.0"},{"v":2,"d":"2.0"},3.5,{"v":382,"d":"382.0"},{"v":458,"d":"458.0"}]
[]
["*： you require another part number please contact with us."]
["**：Inductance Tolerance ± 20% ；Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：Isat : DC current (A) that will cause Lo to drop approximately 30%"]
["Note4：The packing quantity is 300Pcs/ disk"]
{"$rows_empty":9}
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"2213系列规格","index":22,"n_rows":46,"n_cols":6,"rows_kept":46,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,6,5],[25,0,25,5],[26,0,26,5],[27,0,27,5],[28,0,28,4]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺电子科技有限公司"]
["SMD POWER INDUCTORS:           2213Series"]
[]
["Series","A(mm)","B(mm)","C(mm)","D(mm)","E(mm)"]
[2213,"22.00±0.5","22.5±0.5","13.0Max","5.0±0.5","18.6±0.3"]
[]
["Part Number","L0\nInductance（µH）±20%","Heat Rating Current\nIrms(A)","Saturation Current\nIsat ( A )","DCR(mΩ）"]
[{"$nulls":4},"TYP.","MAX."]
["FHW-2213TY-R47M-G/B",0.47,{"v":80,"d":"80.0"},{"v":100,"d":"100.0"},0.56,0.67]
["FHW-2213TY-1R0M-G/B",{"v":1,"d":"1.0"},{"v":69,"d":"69.0"},{"v":71,"d":"71.0"},0.86,0.89]
["FHW-2213TY-2R2M-G/B",2.2,{"v":58,"d":"58.0"},{"v":48,"d":"48.0"},1.22,1.25]
["FHW-2213TY-3R3M-G/B",3.3,{"v":49,"d":"49.0"},{"v":41,"d":"41.0"},{"v":1.5,"d":"1.50"},{"v":1.8,"d":"1.80"}]
["FHW-2213TY-4R7M-G/B",4.7,{"v":47,"d":"47.0"},{"v":37,"d":"37.0"},1.77,1.84]
["FHW-2213TY-6R8M-G/B",6.8,{"v":36,"d":"36.0"},{"v":36,"d":"36.0"},2.84,3.09]
["FHW-2213TY-100M-G/B",10,{"v":28,"d":"28.0"},{"v":28,"d":"28.0"},{"v":3.8,"d":"3.80"},4.14]
["FHW-2213TY-150M-G/B",{"v":15,"d":"15.0"},23.5,{"v":24,"d":"24.0"},5.62,6.11]
["FHW-2213TY-220M-G/B",22,"17.5(30)","16(20)","10.6(9.6)","10.8(13)"]
["FHW-2213TY-330M-G/B",{"v":33,"d":"33.0"},15.5,10.5,{"v":15.1,"d":"15.10"},{"v":15.4,"d":"15.40"}]
["FHW-2213TY-470M-G/B",47,13.5,10.5,{"v":17.3,"d":"17.30"},{"v":17.7,"d":"17.70"}]
["FHW-2213TY-750M-G/B",{"v":75,"d":"75.0"},{"v":12,"d":"12.0"},{"v":12,"d":"12.0"},29.76,32.35]
["FHW-2213TY-820M-G/B",82,10.2,{"v":9,"d":"9.0"},31.46,{"v":34.2,"d":"34.20"}]
["FHW-2213TY-101M-G/B",{"v":100,"d":"100.0"},9.1,{"v":7,"d":"7.0"},36.25,{"v":39.4,"d":"39.40"}]
["FHW-2213P-151M-G/B",150,{"v":6,"d":"6.0"},{"v":8,"d":"8.0"},{"v":68,"d":"68.0"},{"v":90,"d":"90.00"}]
["FHW-2213P-221M-G/B",{"v":220,"d":"220.0"},4.5,{"v":6,"d":"6.0"},{"v":98,"d":"98.0"},{"v":130,"d":"130.00"}]
["FHW-2213P-401M-G/B",400,{"v":4,"d":"4.0"},{"v":6,"d":"6.0"},{"v":208,"d":"208.0"},{"v":270,"d":"270.00"}]
["**：Inductance Tolerance ± 20%   Frequency Test：100KHz/1.0V"]
["Note 1：All test data is referenced to 25℃ ambient."]
["Note 2：Idc : DC current (A) that will cause an approximate△T of 40℃"]
["Note 3：(T)Isat : DC current (A) that will cause Lo to drop approximately 20%"]
["               Isat : DC current (A) that will cause Lo to drop approximately 30%"]
{"$rows_empty":13}
["深圳市丰辉旺科技有限公司"]
["联系电话，18503051681李生"]
["官网；www.jh-dzcl.com"]

{"sheet":"Sheet1","index":23,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}