{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["CH0810-1.5MH "],"not_rendered":{"images":1,"comments":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"CH0810-1.5MH ","index":0,"n_rows":36,"n_cols":10,"rows_kept":36,"merged":[[0,0,0,9],[1,0,1,9],[3,0,3,4],[3,5,3,9],[4,0,4,5],[4,6,4,8],[5,0,15,9],[16,0,16,1],[16,2,16,3],[16,4,16,6],[16,7,16,9],[17,0,17,1],[17,2,17,3],[17,4,17,6],[17,7,17,9],[18,0,18,9],[19,0,19,2],[19,3,19,6],[19,7,19,9],[20,0,20,2],[20,3,20,6],[20,7,20,9],[21,0,21,2],[21,3,21,6],[21,7,21,9],[22,0,22,9],[23,0,23,2],[23,3,23,6],[23,7,23,9],[24,0,24,2],[24,3,24,6],[24,7,24,9],[25,0,25,2],[25,3,25,6],[25,7,25,9],[26,0,26,9],[27,0,27,6],[27,7,27,9],[28,0,28,9],[29,0,29,9],[30,0,30,4],[30,5,30,9],[31,0,31,3],[31,7,31,9],[32,1,32,3],[32,5,32,9],[33,1,33,3],[33,5,33,9],[34,1,34,3],[34,5,34,9],[35,0,40,3],[35,4,35,5],[35,6,35,7],[35,8,35,9],[36,4,40,5],[36,6,40,7],[36,8,40,9],[41,0,41,9]],"flags":["formulas_cached_only"]}
["深圳市丰辉旺科技有限公司"]
["网址；www.jh-dzcl.com;电话；18503051681"]
[]
["CUSTOMER：",{"$nulls":4},"CUSTOMER PART NO："]
["NAME＆OUR PART NO.: PK3W0608-100MH/120UH",{"$nulls":5},"DATE: 2020/07/06",null,null,"REV:A1"]
["1.DIMENSION(UNIT:mm):(外型尺寸单位:mm)"]
{"$rows_empty":10}
["   A: 11.0 MAX",null,"B: 9.5MAX",null,"C:17.0±2.0(PIN2)",null,null,"D: 14.0±2.0(PIN1,3)"]
["   E: ",null,"F: ",null,"G: ",null,null,"H:"]
["2.ELECTRIC CHARACTERISTICS:(电气特性)"]
[" L1-2： 370UH±10%",null,null,"L2-3:120UH ±10%",{"$nulls":3},"TEST FREQ:  1KHZ  0.25V"]
["  N1-2:Ф0.01mm*680TS ",null,null,"N2-3:Ф0.01mm*30TS  "]
[" Q:",null,null,"IDC:    "]
["3.TEST EQUIPMENT:(测试仪器)"]
[" □HP-4284A(LCZ-METER)",null,null,"    ■CH-1062(LCZ-METER)",{"$nulls":3},"□CH-301A(CURRENT METER)"]
[" □HP-8712C(ANALIZER)",null,null,"    □SK-3005(INSULATION TESTER)",{"$nulls":3},"□MQ-1601    (Q-METER)"]
[" □CH-100(LCR-METER)",null,null,"    □CH-852A(HIGH POT TEST METER)",{"$nulls":3},"■TH-2511（DCR METER）"]
["4.MATERIALS LIST:(材料表)"]
["   CORE(磁芯）:F6 DR3W6*8",{"$nulls":6},"PIN(针脚):0.50mm*14mm*17mm"]
["   WIRE（线规）:  Φ0.01mm"]
["   SLEEVE（套管）:   Ф6mm* 10.3 mm  (MARK: PVC COLOR: BLACK    )           m/KPCS"]
["   VARNISH（油漆）:"]
["   TAPE（胶带）:  mm  ＆  mm  ",{"$nulls":3},"N.W:     KG/KPCS",null,null,"  PACKING: "]
[" REV.","REVISIONS  REC.",null,null,"DATE","NOTE: 1.PIN1和PIN3.2有明显长短区别.                                 "]
[{"$nulls":5},"2.PIN1和PIN3长度一样。"]
[]
["APPROVED BY CUSTOMER:（客户承认签回）",{"$nulls":3},"DRAWN  BY",null,"CHECKED  BY",null,"APPROVED  BY"]